Installing Custom HP 630 Media Profiles for SAi FlexiSIGN
---

1. Enter your printer's IP Address in a web browser.  Select Substrate > Substrate Preset Management > Import substrate preset.  Choose the .OMS portion of the profile, and click Import.  Follow the onscreen prompts until the message appears notifying of successful installation.

2. In Production Manager, go to File > Import Preset and select your downloaded .PTF file.

Select the new media Preset when opening a file, setting as the default job or printer properties, and printing.

Note: Using only the .OMS portion of the profile or Auto synchronized print modes without installing/using the .PTF portion of the profile will not result in optimal print results.  The ICC portion of the media profile has been created in SAi for a specific print mode(s) and is installed specifically by the .PTF.  Use of the preset will select the correct Output Profile automatically.  You should not change this selection manually.

Note: Depending on the media, overcoat may be turned on for printing.  If laminating, set the overcoat value of the media to 0 (zero) on the front panel of the printer or select "Optimize for Lamination" in the RIP prior to printing.