Installing Custom HP 700-800 Media Profiles for Onyx
---

1. Enter your printer's IP Address in a web browser.  Select Substrate > Import substrate preset.  Choose the .OMS portion of the profile, and click Import.  Follow the onscreen prompts until the message appears notifying of successful installation.

2. In Onyx RipQueue, select your printer and click "Configure Printer."

3. Select the Media tab and click on the Import button.  Browse to the extracted .OML file.  A dialog will appear which allows you to choose the media. Select the media and choose Import.  The media profile is now available for use in Onyx.

Note: Using the .OMS portion of the profile or Auto populated print modes without installing/using the .OML portion of the profile will not result in optimal print results.  The ICC portion of the media profile has been created in Onyx for a specific print mode(s) and is installed specifically by the .OML.

Note: By default, overcoat is turned on for printing.  If laminating, set the overcoat value of the media to 0 (zero) on the front panel of the printer prior to printing.