Installing Custom HP 700-800 Media Profiles for Caldera
---

1. Enter your printer's IP Address in a web browser.  Select Substrate > Import substrate preset.  Choose the .oms portion of the profile, and click Import.  Follow the onscreen prompts until the message appears notifying of successful installation.

2. In Caldera EasyMedia, choose Import > Install Patch.  Choose the .calpatch portion of the profile and click Install.

The profile is now ready for use.  Note you may need to stop/restart the Caldera printer server for updates to take effect.

Note: Using the .OMS portion of the profile or Auto synchronized print modes without installing/using the .calpatch portion of the profile will not result in optimal print results.  The ICC portion of the media profile has been created in Caldera for a specific print mode(s) and is installed specifically by the .calpatch.

Note: By default, overcoat is turned on for printing.  If laminating, set the overcoat value of the media to 0 (zero) on the front panel of the printer prior to printing.