Installing media profiles for Mimaki RasterLink Pro III

1. Extract the ICC profile from the downloaded .zip file
2. Open Mimaki Raster Link ProIII > ProfileManager
3. Select Profile > Install Device Profiles.
4. Browse to the folder containing the profile that you just extracted and OK.  You will see the name of the profile in the top of the next window that appears.  Select it, click the down arrow button and OK.  The profile will be installed and available for use when you re-launch RasterLink ProIII

To apply the profile:
1. Open a job, right click on it in the Job List and choose Edit.
2. Select the Print Condition tab, and under Media, select the top listing and choose the name of the profile that was just installed.  A list of available print modes will appear below.
3. Select the mode of the profile you wish to use.  You will see the settings in the Print mode tab change to those included and recommended for the profile.
4. Select the Condition Management button in the bottom right of the Job Editor window.
5. Select your printer > select the Print Condition tab > Update With Job > Close.
6. Select OK in the Job Editor window.

The profile will now apply when you RIP & Print the job.  This profile will also be the default for newly added jobs until the printer's Print Condition is changed.

The recommended print mode settings such as resolution, pass count, heater settings, print direction, etc. will be automatically set when using this profile in the method described above.