Installing ColorBurst v9.2 Media Profiles
---
1. Extract the folder containing the General Formulations ColorBurst v9.2 files (ex: media_name.lin, media_name.icc, and General Formulations folder) from the downloaded ZIP file.

2. Close ColorBurst v9.2 if running, and open Windows Explorer (right click on the Windows Start button > Explore).  Navigate to the location your ColorBurst RIP is installed (ex: C:\ColorBurst_9.2 GS6000).

3. Move the .lin file into the "Lin" folder, and move the .icc file into the "Profiles\Output" folder.  Move the downloaded "General Formulations" folder inside the ColorBurst "Env\EM_Epson\EM_Epson GS-6000" folder.

*NOTE: If you have previously installed a General Formulations media profile, and the "General Formulations" folder already exists, you can move only the General Formulations/Media Name sub-folder into the pre-existing "General Formulations" folder.

4. Exit Windows Explorer and launch ColorBurst to configure your profile.


Configuring your Media Profile
---
1. In ColorBurst, click on the "Environments" button, scroll down to General Formulations, and select your media environment.

Note: You may receive an error when first selecting the new environment.  Click OK and follow the steps below.

2. Click on the "Linearization Options" button, the "Select a lin file" button in the next window, then open the .lin file that you just installed.

3. Next, click on the "ICC Profile Options" button. Under the Output Profiles tab, click the On/Off button (the Find button will now become active), click Find, then open the .icc profile that you just installed.

4. Resave the Environment (Environments > Save As... > OK).