Installing HP 500 Series Onyx Media Profiles
---

Note: the printer OMS portion of the profile is embedded in the Onyx OML file and will be installed as noted below.

1. Extract the profile (.OML) from downloaded Zip file.

2. In Onyx RipQueue, select your printer and click "Configure Printer."

3. Select the Media tab and click on the Import button.  Browse to the extracted .OML file.  A dialog will appear which allows you to choose the media. Select the media and choose Import.  The media profile is now available for selection in Onyx.

4. On first use of the profile (when hitting the Print Now button), Onyx will syncronize with the printer and you will be prompted to upload the media to the printer.  Click Yes in Onyx, then "Continue" on the front panel of your printer when prompted.  Once the printer panels shows that installation is succesful, select the media on the printer.  The profile is now fully installed in both the RIP and the printer and you may use the profile as normal going forward.