Installing Custom HP 700-800 Media Profiles for SAi FlexiSIGN
---

1. Enter your printer's IP Address in a web browser.  Select Substrate > Import substrate preset.  Choose the .OMS portion of the profile, and click Import.  Follow the onscreen prompts until the message appears notifying of successful installation.

2. In Production Manager, go to File > Import Preset and select your downloaded .PTF file.

Select the new media Preset when opening a file, setting as the default job or printer properties, and printing.

Note: Use of the preset will select the correct Output Profile automatically.  You should not change this selection manually.

Note: By default, overcoat is turned on for printing.  If laminating, set the overcoat value of the media to 0 (zero) on the front panel of the printer prior to printing.  Alternately, this can be set in SAi Production Manager under Job Properties/Default Job Properties > Printer Options Tab by checking the "Optimize for lamination" box.